**"HETEROTOPIES. BOTEVGRAD - LESKOVAC" UNDER INTERREG-IPA CROSS-BORDER COOPERATION PROGRAM BULGARIA-SERBIA**

|  |  |  |  |
| --- | --- | --- | --- |
| **CLOCK TOWER** | | | |
| **TECHNICAL SPECIFICATION** | | | |
|  | |  | **ELECTRIC LADDER**  L90 cm, B64 cm, H51 cm, / unfolded position /  L90 cm, B15 cm, H69 cm, / stowed position /  mobile module with electric drive with steps for access to the tower, rail movement, cantilever, with dimensions according to the architect's scheme and control measure from the place  load-bearing structure steps - carbon or low-alloy steel, L profile, powder coated,  fasteners - galvanized, powder coated metal parts processing - gray granular coating with light wavy surface for increased scratch  resistance flooring - oak board L90 cm, B30 cm, H3cm with a tooth to cover the metal structure / from the material of the flooring in the tower /, deep impregnation for 30 years of protection from weathering, insecticides and fire. |
|  | **PLATFORM FOR PEOPLE WITH DISABILITIES**  Delivery and installation of a vertical platform type "Liftboy" for people with disabilities - 750x900 mm / maximum load capacity 180 kg, lifting height maximum 595 mm, lifting height minimum 100 mm/,  manual and automated control, platform floor covering - metal parts processing - gray grain coating with light wavy surface for increased scratch resistance  wooden oak cladding for wooden floors / protection from weathering, insecticides and fire. |
|  | | | **BRIDGE**  L725 cm, B160 cm, H40 cm, Delivery and installation of a bridge  metal supporting structure, for the wooden surface - stainless steel, closed profile 30x30mm, welding installation, powder coated,  fasteners for mounting on wood on steel and on wood on wood - stainless steel, powder coated, mounting with hidden screw heads - from mounting system decking  timber first category according to BDS427, FSC / PEFC certified, maximum humidity 12%  whips - 3 pieces, longitudinally in 40 cm  L725cm, B4.5cm, H9cm, mounting on a metal structure  Siberian larch flooring type decking wholesale corrugated, density 700 kg / cubic meter, plank size  L150 cm, B14 cm, H3 cm, installation of a plank on a bar - at a distance - to absorb deformations / swelling and drying /, for ventilation and fast drying, deep impregnation for 30 years of protection from weathering, insecticides and fire.  **Mandatory!**  control measures from gauge space |
| кота 14.65    кота 0.00 | от кота 14.65 до кота 21.50 | | **PERISCOPE**  Periscope system - complex facility in two modules  Module 1 for assembly and installation at an altitude of elevation 14.65 to elevation 21.50 / camera - under the bell, metal piping powder-polymer coating, display, integrated network module, thermostated system /  Associated with Module 2 for assembly and installation of monitor system at elevation 0.00 / display - 43 "multi-touch, integrated control computer, integrated network module, protective impact-resistant coating, housing - metal with powder-polymer coating, thermostated with built-in air conditioning system, providing operation at temperatures of -10 \* C to + 45 \* C, IP 65 /, incl. system testing |

**ARCH. MARIELA ANDREEVSKA**